##############################################################
#
# Xilinx Core Generator version 11.2
# Date: Fri Jun 12 05:42:56 2009
#
##############################################################
#
#  This file contains the customisation parameters for a
#  Xilinx CORE Generator IP GUI. It is strongly recommended
#  that you do not manually alter this file as it may cause
#  unexpected and unsupported behavior.
#
##############################################################
#
# BEGIN Project Options
SET addpads = False
SET asysymbol = False
SET busformat = BusFormatAngleBracketNotRipped  
SET createndf = False
SET designentry = vhdl
SET device = xc6slx45
SET devicefamily = spartan6
SET flowvendor = Foundation_ISE
SET formalverification = False
SET foundationsym = False
SET implementationfiletype = Ngc
SET package = csg324
SET removerpms = False
SET simulationfiles = Structural
SET speedgrade = -3
SET verilogsim = False
SET vhdlsim = False
# END Project Options
# BEGIN Select
SELECT VIO_(ChipScope_Pro_-_Virtual_Input/Output) family Xilinx,_Inc. 1.03.a
# END Select
# BEGIN Parameters
CSET asynchronous_input_port_width=8
CSET asynchronous_output_port_width=7
CSET component_name=vio
CSET enable_asynchronous_input_port=false
CSET enable_asynchronous_output_port=true
CSET enable_synchronous_input_port=false
CSET enable_synchronous_output_port=false
CSET invert_clock_input=false
CSET synchronous_input_port_width=8
CSET synchronous_output_port_width=8
# END Parameters
GENERATE
# CRC: 66fe39ed

